|  |  |  |
| --- | --- | --- |
| |  |  | | --- | --- | | |  | | --- | | **Digitest® 3: Best Practices and Common Mistakes to Avoid.** | | |
| |  | | --- | | [**Digitest® 3**](https://parkell.eu/product/pulp-vitality-tester/) is built to **simplify**pulp vitality testing while ensuring **reliable results**. Even so, regular care is key to keeping it **accurate** and **performing well**. We’ve  Compiled some tips to help you maintain your device and achieve optimal **results.** | |
| |  |  | | --- | --- | | |  | | --- | |  | | |
| |  |  | | --- | --- | | |  | | --- | | **Best Practices** | | |
| |  |  | | --- | --- | | |  | | --- | | * Pair pulp testing with x-rays, hot/cold, or percussion for complete diagnostics. * Keep probes and clips spotless according to our [IFU](https://parkell.eu/wp-content/uploads/2025/04/Digitest3_EU_ifu_multi.pdf). * Use **Digitest® 3** accessories with confidence, even on older Digitest models. * Protect the power unit by cleaning with wipes under 30% alcohol, or alcohol-free disinfectants. | | |
|  |
| |  |  | | --- | --- | | |  | | --- | | **What to Avoid?** | | |
| |  |  | | --- | --- | | |  | | --- | | * Using **Digitest® 3**with patients who have pacemakers, defibrillators, or insulin pumps. * Using accessories from other third-party pulp. * Soaking, spraying, or machine-washing the power unit. | | |
| |  | | --- | |  | |
| |  |  | | --- | --- | | |  | | --- | | Simple habits can have a big impact on your device’s accuracy and longevity. Discover how to achieve reliable, lasting results. | | |