|  |  |  |
| --- | --- | --- |
|

|  |  |
| --- | --- |
|

|  |
| --- |
| **Digitest® 3: Best Practices and Common Mistakes to Avoid.** |

 |

 |
|

|  |
| --- |
| [**Digitest® 3**](https://parkell.eu/product/pulp-vitality-tester/) is built to **simplify**pulp vitality testing while ensuring **reliable results**. Even so, regular care is key to keeping it **accurate** and **performing well**. We’ve Compiled some tips to help you maintain your device and achieve optimal **results.**  |

 |
|

|  |  |
| --- | --- |
|

|  |
| --- |
|  |

 |

 |
|

|  |  |
| --- | --- |
|

|  |
| --- |
| **Best Practices** |

 |

 |
|

|  |  |
| --- | --- |
|

|  |
| --- |
| * Pair pulp testing with x-rays, hot/cold, or percussion for complete diagnostics.
* Keep probes and clips spotless according to our [IFU](https://parkell.eu/wp-content/uploads/2025/04/Digitest3_EU_ifu_multi.pdf).
* Use **Digitest® 3** accessories with confidence, even on older Digitest models.
* Protect the power unit by cleaning with wipes under 30% alcohol, or alcohol-free disinfectants.
 |

 |

 |
|  |
|

|  |  |
| --- | --- |
|

|  |
| --- |
| **What to Avoid?** |

 |

 |
|

|  |  |
| --- | --- |
|

|  |
| --- |
| * Using **Digitest® 3**with patients who have pacemakers, defibrillators, or insulin pumps.
* Using accessories from other third-party pulp.
* Soaking, spraying, or machine-washing the power unit.
 |

 |

 |
|

|  |
| --- |
|   |

 |
|

|  |  |
| --- | --- |
|

|  |
| --- |
| Simple habits can have a big impact on your device’s accuracy and longevity. Discover how to achieve reliable, lasting results. |

 |

 |